Delay

Make GPIO pin high or low

Compare command with reference

Fetch commands from server

Connect to server through API

Connect to wifi

search for wifi network